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Thermostat

The thermostat is integrated in the thermostat housing,
which is mounted directly on the cylinder head. Inside the
thermostat housing there are two thermostats for the
twin-circuit cooling system.

Thermostat 1

Opens from approximately 188 °F (87 °C) and allows
coolant to flow from the radiator to the coolant pump.

Thermostat 2

Opens from approximately 217 °F (103 °C) and allows
heated coolant to flow from the cylinder block to the radia-
tor. The entire coolant circulation system is open.
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